-----------------------------------------

For technical details related to the sonar device please contact:

Dr. Somasundar Kanan (s.kannan1@rgu.ac.uk)

1. Open Folder named CSV

---------------------------------

If you open any csv file -

First column is angles, scanned from 100 - 300 forward scan 180 degrees.

Each row corresponds to the sample responses of sonar. There will be 1200 responses for each angle, thus the sample rate is 1200.